-----------------------------------------------------------------------------------------------------------------------------
Important:
Please use your local cards in newcamd-client.txt on buttom..also as last in file.
This will guarantee that all the time first your cards are used and as second choice
spider or another routes,think on traffic please 
N2 idea key must be as N prov 00 idea key in Keylist.txt
Tps key must be as T:xxxxxxxxxxxxxxxxxxxxxxxxxxxx in /var/keys/tps
Biss keys must be as B sid 00 xxxxxxxxxxxxxxxxxxxxxxxxx in Keylist.txt(same for static cw providers)
NDS emm is 100% tested and should work for all available providers.
Nagra2 key format is changed since Version 1.06( where AU code for nagra2 was added) :
Format:

; N2 Keys:
; M1 - ECM RSA Modulus (e = 3)
; N1 - EMM RSA Modulus (Round 1, e = 3)
; PK - EMM Parity Key (Expanded to N2 and E2) or I - idea key
; V - EMM Verify Key

-----------------------------------------------------------------------------------------------------------------------------


Evocamd-Next Level version 2.00
-------------------------------
 As evocamd now uses enigma specific socket messages, it was not possible to keep all machines in one binary.
 From now on you will find some extra directories for binaries.
 - dreambox_7025
 - dreambox_ppc
 - dragon
 - relook
 - dbox
 New is the mipsel(7025) and ppc Dream binaries. You will now be able to watch one channel and record more 
 channels at the same time, and this without any changes in enigma source. No patch is needed for this.
 On 7025 you will be able, with two tuners to record two channels and watch a third at the same time(dunno any CI that can do this :P)
 On 7020 or 7000 you must enable in CI menu "can handle two services", you are then able to record one
 channel and watch another at the same time, but note this is only possible on the same Transponder.
Camd3 client old proto is enabled again, so you can use it to talk with dukat or freezers servers around :)
Radegast client is enabled too, and tested.
-------------------------------------------------------
Important!

Few words about multichannel, please keep in mind that not all cards suport too many requests same time, and please
if you use some Spider Network dont use it just for fun..use it just if needed as you will make higher traffic in net.


In diese Distribution befinden sich mehrere binaries für verschiedene boxen wie folgt:
- dreambox_7025
- dreambox_ppc
- dragon
- relook
- dbox

Neu ist die dreambox 7025 binarie mit multichannel support ( es ist möglich zum Beispiel zwei channels aufzunehmen und ein drittes
zu gucken)
Das gilt auch für die ppc Version mit die aber nur ein channel aufnehmen und eins gucken auf den Selben Transponder möglich ist.
Dafür aber die entsprechen option in CI menu aktivieren.
Camd3 client wurde wieder aktiviert ( das alte protokoll), damit könnte man auf Dukat oder freezer Servers verbinden.
Radegast client ist auch so weit aktiviert aber leider noch nicht getestet. 
--------------------------------------------------------
Wichtig!
Bitte denkt daran das drei requests gleichzeitig nicht von alle karten Unterstützt wird, und das macht
unnötige Traffic in Zb Spider Net, also bitte nur benutzen wenn unbedingt notwendig.
camd3 config syntax :
camd35:bla.linux.net:20248:1/1702:test1:test1
in "/var/keys/camd35.conf"

Evocamd-Next Level version 1.10
-------------------------------
fix AU problem on nagra2 channels (USA)
fixes freezing/pixelation problems people have been seeing on nagra2

Evocamd-Next Level version 1.09
-------------------------------

fix cabo n2 ident


Evocamd-Next Level version 1.08
-------------------------------

fix swap of dcw on nagra2 providers

Evocamd-Next Level version 1.07
-------------------------------
"autofetch AES Key feature"

Location of aes key was changed to /var/keys/tps.
If file not present will be created.
To update your aes key you must put in camd_cfg URL from 
where to fetch the new one.
Example:
wwwtps = http://xxxxxxxxxxxxxxx/SoftCam.Key
Important:
Just SoftCam.Key format will be used.

Kleine änderung:
tps key wird jetzt in /var/keys/tps erwartet.
Falls file nicht existiert, es wird angelegt und mit gültige key ausgefüllt
soweit in camd_cfg dieser Eintrag existiert:
wwwtps = http://xxxxxxxxxxxxxxx/SoftCam.Key
Nur SoftCam.Key format wird unterstützt für autofetch!!!

Fehlerhafte libcrypto wurde in Package ersetzt.

Evocamd-Next Level version 1.06
-------------------------------
Nagravision2 autoroll for some providers ( Dish, Bev)
thx an bball for support.
Added new binary for relook pvr
Vdr binary updatet

Evocamd-Next Level version 1.05
-------------------------------
BEV Canada fix

Evocamd-Next Level version 1.04
-------------------------------

Nagravison2 emm handling added.

Evocamd-Next Level version 1.03
-------------------------------

Videoguard Multiple EMM handling added.
Changed to libcrypto.so.0.9.7 instead of libcrypto.so.0


Evocamd-Next Level version 1.02
-------------------------------

Some small needed fixes.
Italia emm is tested and should work okay now.

Evocamd-Next Level version 1.01
-------------------------------

Nagra AU fix
Italia emm fix(videoguard)

Evocamd-Next Level version 1.00
-------------------------------

evocamd_ppc.bin			->	Evocamd binary for dreambox
evocamd-oldGCC.bin		->	Evocamd with support for Triple Dragon and Dbox2(old gcc)
directory /vdr			->	Evocamd binary for VDR + evo-vdr-1.3.21.diff

Konfiguration(Configuration) Files
-------------------

camd_cfg
Autoupdate.Key
Keylist.txt
newcamd-client.txt
ignore.list
priority.list
replace.list
eeproms und rams(siehe scce Ordner)

------------------------------------------------------------------------------------------------------------------------------


Ja genau, wir haben endlich geschaft evocamd neu zu designen.
Warum?Nun dort waren viele sachen womit wir mehr oder weniger nicht Zufrieden waren.
Was hat sich geändert?
NewCS client wurde überarbeitet um best mögliche speed zu erzielen,das gleiche gilt 
für emu modus ..jedoch immer daran denken "priority.list ignore.list replace.list " zu konfigurieren(Beispiel Datei liegt bei).
Warum werden diese dateien benutzt?Es ist in eure Interesse Leute !!!Damit habt ihr unbegrenzte möglichkeiten
in was ecm pids oder provider Auswahl betrifft.Denke nicht das besser wäre wenn wir das für euch bestimmen, ein 
bisschen flexibilität wäre dann nicht mehr vorhanden.
Ausser NewCS wird noch radegast share Ünterstützt, jedoch die camd3 Unterstützung wurde eingestellt, da wie wir verstanden haben
Änderungen in protokoll gegeben haben soll.
-------------------------------------------------------------------------------------------------------------------------------


Welche Syteme werden Unterstützt:
Emulation:
---------
Seca - ecm
Viacess - ecm & emm
Irdeto - ecm & emm
Biss - ecm
Nagravision - ecm & emm(nur n1)
-------------------------------------


Card Support trough NewCS cardserver:
-------------------------------------
 *- Conax       *- Seca        
 *- Irdeto      *- Cryptoworks 
 *- Betacrypt   *- Viaccess    
 *- Dreamcrypt  *- Videoguard  
-----------------------------------------------------------------------------------------------
NOTE!
EMM IST SUPPORTED FÜR ALLE CA-SYS(siehe oben) ausser dreamcrypt!!!!!!
FALLS IHR SOGENANNTE MOSC CARDS BENUTZT, BITTE VORHER BLOCKER IN NEWCS CONFIG AKTIVIEREN.
WIR SIND NICHT VERANTWORTLICH FÜR MÖGLICHE SCHADEN,SPRICH KARTE DEAKTIVIERT DURCH PROVIDER !!!
-----------------------------------------------------------------------------------------------
 







WICHTIG
--------

In Radegast share wird clear modus sharing unterstützt sowie crypted !!!
Für benötigte Einstellungen, bitte rdgd readme beachten	
Um OSD benutzen zu können wurde die camd_cfg erweitert mit USER = und PWD = einstellungen. 

Faq

1. Its support evocamd tps2 channel?
Indeed,just put your aes key in Autoupdate.key
T: xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

2.Its sharing possible with evocamd?
Yes,you can use the spider net and NewCS/cardserver
3.Can i use my cards in dream or Triple dragon slots?
Offcorse,just setup a newcamd cardserver,and put your login Data in newcamd-client.txt
4.Is emm supported with newcamd-cardserver?
Yes,irdeto-conax-seca,cryptoworks,viacess is supportet,just setup one AU user in cardserv.cfg and you are done
5. Is a premiere card supported with evocamd?
Offcorse, NewCS rulez :)))))))

7.I get AU on  Cabo but i dont have picture,and in log i see mecm failed
Check in Autoupdate.key if e1n and n1n are corect
8.Can i use my premiere card in dbox2 normal slot?
Yes,you can
9.How can i log on my windows pc?
In camd_cfg you must setup one UDP port for logging, you find a client in our distribution
10.I cant use camd3 client with a dreamcrypt card
Its must work,but please check allways your ignore.list,maybe you ignore some caids or provider what you need