Speedy Handbook 0.4 for S

////////////////////////////////////////////////////////////////////////////////

Welcome to the Speedy Conexant experience, welcome to the S by GXMax

Howto
-----
1. Upload .ups
2. Go to "UTILITY", "USB" and select scam-x.xx.exx file in order to upload emulator module
3. Go to "UTILITY", "USB" and select updated softcam.key (you can download it from Internet)
4. Enjoy

TPS AU
------
Tune Hotbird 10873 transponder for AES AU, for example M6 Music Rock channel

Direct keys from Internet
-------------------------
Configure your network settings if not done yet
Press "page down" key to open window for network keys
Input url if needed
Press update button

Nagra2 smartcard
----------------
Load a bk.txt file with your card data:
  - First 8 bytes are boxkey
  - Following 24 bytes are key0D

Backup keys
----------------------------
If you want to backup your keys, you can store it from receiver to usb:
Go to "UTILITY", "USB" and press blue key ("save key") in order to create your own softcam.key file

Everytime you upload an scam.exx file to receiver, keys will reset to default

Filetypes
---------
.ups - main software
.exx - modules
.sdb - channels lists
.key - softcam keys

////////////////////////////////////////////////////////////////////////////////

The GXMax team
