Josje01 ToH3.4Hot10.2NLgemonteerd.hdf
CRC: 61468372
MD5: acb3efcd590e37836a24db8cfa35e6c1

Many thankx to PH/HoT


Humax ToH3.4 HoTplugged v10.2 - 2008-02-04
-- Version: A --
============================
- TPS AU Fix 

Humax ToH3.4 HoTplugged v10.1 - 2008-01-25
-- Version: A --
============================
- Polsat AU Fix 
- DigiTV AU Fix
- PW AU on Betacrypt (1702)


HoTplugged v10.0 - 2008-01-17
-- Version: A --
============================
- Polsat AU Fix
- small Fixes


HoTplugged v9.9 - 2008-01-05
-- Version: A --
============================
- PW AU Fix
- new Config Option Nagra2 AU
  o AUTO (Default) = AU only if necessary (Expired Keys)
  o ON = AU always 
  o OFF = AU disabled
 

don’t need to be converted for Humax 5400Z Plus!


HoTplugged v9.8 - 2007-12-20
-- Version: A --
============================
- PW Direkt/BlueMovie Fix 

HoTplugged v9.7 - 2007-12-05
-- Version: B --
============================
- PW AU Freeze Fix 

HoTplugged v9.7 - 2007-12-04
-- Version: A --
============================
- PW AU Fix 

Humax ToH3.4 HoTplugged v9.6 - 2007-11-21
-- Version: A --
============================
- Polsat AU Fix 
- TPS GMT Fix (summer/winter)
- D+ AU Fix
  Please notice that D+ AU is very processor intensive,
  therefore the Humax freeze during AU. AU need up to 
  5 Minutes. You must turn off and on to get AU.


Humax ToH3.4 HoTplugged v9.5 - 2007-09-09
-- Version: B --
============================
- Polsat AU Fix 
- biss detection fix for L1.37

Humax ToH3.4 HoTplugged v9.5 - 2007-09-07
-- Version: A --
============================
- Polsat AU 
(many THX to Mahdi)

Humax ToH3.4 HoTplugged v9.4 - 2007-09-05
-- Version: A --
============================
- Pixelerror Fix
- new structure for biss 
  frequency (Tolerance +/- 6) + SID (last Byte) + PMT (last byte) + key
  compatibel to SAMSUNG
- EMU moved to Module 4
- ORF Nagra Support
- Localia (30°W) Nagra Support (not tested)
- DigiTV AU

Humax ToH3.4 HoTplugged v9.3 - 2007-08-27
-- Version: A --
============================
- TV CABO AU Fix
- D+ AU Fix
- DigiTV Fix


Humax ToH3.4 HoTplugged v9.2 - 2007-08-19
-- Version: A --
============================
- TV CABO AU 
  please remove CAM while updating

Humax ToH3.4 HoTplugged v9.1 - 2007-08-13
-- Version: A --
============================
- D+ AU 
  please remove CAM while updating

Humax ToH3.4 HoTplugged v9.0 - 2007-08-12
-- Version: B --
============================
- PW AU fixed and enabled 

Humax ToH3.4 HoTplugged v9.0 - 2007-08-12
-- Version: A --
============================
- PW AU disabled  


Humax ToH3.4 HoTplugged v8.9 - 2007-08-11
-- Version: A --
============================
- Buli BugFix  


Humax ToH3.4 HoTplugged v8.8 - 2007-08-07
-- Version: A --
============================
- Showtime 7°W AU  
  (many THX to Mahdi, HNAGA and G++)


Humax ToH3.4 HoTplugged v8.7 - 2007-08-01
-- Version: B --
============================
- CAM FiX for TPS 

Humax ToH3.4 HoTplugged v8.7 - 2007-07-30
-- Version: A --
============================
- TPS AU on 10873 V (France4, France5)
  wait about 15 sec.
  tps.hdf disabled (no longer needed)
  (many THX to Mahdi).


Humax ToH3.4 HoTplugged v8.6 - 2007-07-23
-- Version: A --
============================
- TPS Fix (no AU yet)

 You just need to make a tps.hdf out of keyset.bin
 from TPS_Files_pack and load it into the Humax
 (on a daily basis). The first time you switch to
 TPS after startup, it will take some seconds to
 build the st20-Emualtor. Be sure that the time
 is set to GMT +2 (Central-Europe). 
 (many THX to Mahdi).

- Catone fix 3.2 included 

- Polsat key0/1 fix

- new bugs :)

thx also to Lombardo for the helpful bug list
	

Humax ToH3.4 HoTplugged v8.5 - 2007-07-16 
-- Version: A --
============================
- CAM-Support on CARD-EMU Mode

Humax ToH3.4 HoTplugged v8.4 - 2007-07-11 
-- Version: A --
============================
- Progress Bar on EPG info Panel

Humax ToH3.4 HoTplugged v8.3 - 2007-06-27 
-- Version: A --
============================
- Audioselection  fix

P.S.
forgotten: thx for G++ for the Turner RSA ;)

HoTplugged v8.2 - 2007-06-26 
-- Version: B --
============================
K*b*l Deutschland fixed
Absat (tps.bin) fixed

Humax ToH3.4 HoTplugged v8.2 - 2007-06-23 
-- Version: A --
============================
- Irdeto Card fix
- PMCT included (Transponder Update)


Humax ToH3.4 HoTplugged v8.1 - 2007-06-21 
-- Version: D --
============================
- VH1 & MTV Esp fix

Humax ToH3.4 HoTplugged v8.1 - 2007-06-20 
-- Version: C --
============================
- Tu*rner, S*yL*nk, K*b*l Deutschland included
- HSIC fixed

HoTplugged v8.1 - 2007-06-16 
-- Version: B --
============================
- D+ AU failed, disabled

HoTplugged v8.1 - 2007-06-16 
-- Version: A --
============================
- MECM60


(no PMCT included)
Humax ToH3.4 HoTplugged v8.0 - 2007-02-12 
-- Version: A --
============================
- D+ AU
- PW AU 

(no PMCT included)


Humax ToH3.4 HoTplugged v7.9 - 2007-01-02 
-- Version: A --
============================
- TP$ Fix 

(no PMCT included)

Humax ToH3.4 HoTplugged v7.8 - 2006-12-24 
-- Version: A --
============================
- TP$ Fix 

TP$.BIN can be loaded via hdfbin-3-006000.raw
(that raw can't be bigger then 0x9F00 bytes!)
time must be set correct (GMT) to get right TP$-key 


(no PMCT included)

Humax ToH3.4 HoTplugged v7.7 - 2006-12-01 
-- Version: A --
============================
- Cryptowork Fix 
- new structure for biss 

exp: Rai Asia ON HOTBIRD
SID = 2136
PMT = 0100
PCR = 00C8
key = 1122334455667788
SID + PMT last byte + PCR last byte + key
213600C81122334455667788

(no PMCT included)

Humax ToH3.4 HoTplugged v7.6 - 2006-09-09 
-- Version: B --
============================
- AES TPS Autoroll

Humax ToH3.4 HoTplugged v7.5 - 2006-05-26 
-- Version: A --
============================
- CW RSA Fix

Please Note:

When Using DSR 9500 EMU, Set "Humax Def", and Verify
from Box to "ON" in "?-context", always zap to a FTA-Channel
first or remove Card.

Please use Card+EMU (in TOH-Config) if you are not using CW-Sharing !
Please set Card Blocker to ECM+EMM if using a Dummy-Card !



Humax ToH3.4 HoTplugged v7.4 - 2006-05-24 
-- Version: A --
============================
- adapted to DSR 9500 EMU Ed54_CW.exe:
	Cryptoworks/BISS/fix CW/ loaded from key.bin
- DD Radio Fix

! old key.bins are not supported anymore

Humax ToH3.4 HoTplugged v7.3 - 2006-05-09 
-- Version: A --
============================
- CW included:

	EasyTV		ok

Humax ToH3.4 HoTplugged v7.2 - 2006-05-08 
-- Version: B --
============================
- CW freezing Fix


Humax ToH3.4 HoTplugged v7.2 - 2006-05-07 
-- Version: A --
============================
- CW included:

	DMC15°W		not tested
	JSTV		ok
	Kingstone	not tested
	Digiturk	nok
	Xtramusic	ok
	Turner		not tested
	Czech Link	not tested
	British Telecom	not tested
	Slovak Link	not tested


Humax ToH3.3 HoTplugged v7.0 - 2006-03-16 
-- Version: A --
============================
- N2 keys via key.bin

modify N2-RSA by keybin (NAGRA, PROVID):

   ecmMod[0x40]	 	= key 0 - 7
   ecmIkey[0x10] 	= key 8 - 9
   ecmIkey9x[0x10]	= key 0xA - 0xB
   ecmVkey[0x10]	= key 0xC - 0XD



Please: We need from the developer of Samy_Humy_Edit 
and/or DSR 9500 EMU Ed a new program version with more then
5 NAGRA-Provider. (20 would be great!) Please contact us on 
http://www.toh.humax-zone.tv/board/

We can't enlarge the number of providers in emu until we have
a new version of editor. :-/
Please we don't want release emu-versions with build-in keys in the
future. So this is very important to get a new keyedit-version !!!


Humax ToH3.3 HoTplugged v6.9 - 2006-03-12 
-- Version: A --
============================
- N2 Globecast added
- N2 Polsat added


Humax ToH3.3 HoTplugged v6.8 - 2006-02-14 
-- Version: A --
============================
- Bugfixes


Humax ToH3.3 HoTplugged v6.7 - 2006-02-03 
-- Version: A --
============================
- N2 TV CABO added



Humax ToH3.3 HoTplugged v6.6 - 2006-01-24 
-- Version: A --
============================
- D+ Fix 


Humax ToH3.3 HoTplugged v6.5 - 2006-01-09 
-- Version: B/C --
============================
- PMCT adjusted 
- bugfixes


Humax ToH3.3 HoTplugged v6.5 - 2006-01-04 
-- Version: A --
============================
- D+ Fix


Humax ToH3.3 HoTplugged v6.4 - 2005-12-24 
-- Version: A --
============================
- SSSP-Mode (gbox)

Humax ToH3.3 HoTplugged v6.1 - 2005-11-27 
-- Version: A --
============================


Humax ToH3.3 HoTplugged v6.2 - 2005-12-04 
-- Version: A --
============================
- Nagra AU disabled
- MTV-CW's


Humax ToH3.3 HoTplugged v6.1 - 2005-11-27 
-- Version: A --
============================
- Card Blocker included
  Use Option ECM/EMM for Dummy-Cards (recommended)
- Portal Fix
- some Bug-Fixes


Humax ToH3.3 HoTplugged v6.0 - 2005-11-20 
-- Version: A --
============================
- AES-Fix (Key 3 and 0x13)
- constant CW can be stored by 2 entries via PMCT like
  IDENT VPID CAS nnnn nnnn nnnn nnnn 0000 (=CW even)
  IDENT VPID CAS nnnn nnnn nnnn nnnn 0000 (=CW Odd)
  (untested)

Humax ToH3.3 HoTplugged v5.9 - 2005-10-23 
-- Version: A --
============================
- Cabo-AU Fix (Key0+1 OK - Key2+3 NOK)
- BISS included (Discovery dosn't work - don't know why)
  use PMCT to modify CWs
  IDENT VPID 2600 nnnn nnnn nnnn nnnn 0000
- EPG/PMCT-Menu use white Button to insert line instantly
- included CAToneV23-Parser
- AES-Key now on Key 3 and 0x13

thx to scriptors and GioppyGio 


Humax HoTplugged v5.8 - 03.09.2005 
-- Version: D+ is back :-) --
============================
- D+ MTV ESP Astra Fix
- DISH Network 61.5°W (ID 0101 - not tested) 


Humax ToH3.3 HoTplugged v5.7 - 27.08.2005 
-- Version: D+ is back :-) --
============================
- D+ Fix (maybe not for long time)

special thanks to:
humax hdl-Team for the code
st20tp2 for support & some pseudo C porting
siko-SK for firmwares rom & ramdump
remote, Nightshad & all people that help humax to extract algo...


Humax ToH3.3 HoTplugged v5.6 - 20.08.2008 
-- Version: Benedikt XVI  --
============================
( 20.08.2008 PMCT Bug-Fix because MCM)
 - MTV/VH1 on Astra Hack 
  (006A without Nano 5105)


Humax ToH3.3 HoTplugged v5.5 B
==============================
- Mediapark Fix

Humax ToH3.3 HoTplugged v5.5
============================
- PW Portal Fix (by Padawan)
- Nagra optimization
- Spice Fix


Humax ToH3.3 HoTplugged v5.4
============================
not released  



Humax ToH3.3 HoTplugged v5.3
============================
- Cabo Fix
- Irdeto Card-Fix


Humax ToH3.3 HoTplugged v5.2
============================

- ORF fix when PW-Card is used
- PK0 AU (Nagra) on Key2+3 (wait some minutes)
- tps crypt optimized
- version 2.1 of CATONE Conditional Access Tool included (thx to that team)

thx also to Humax & D-Mon



HoT



CATone V3.2


file CRC: 2AF7FC9B
file MD5: 832e89cf7a5e62fbb77bb316c0aa511f

History and changes

CATone V3.2
- Crytoworks provider name list updated
- Nagra current keyset bugfix

CATone V3.0
- Unlimited Number of BISS/Fixed CW Keys (up to key bin size!) 
  (multiple pressing Radio Button will show additinal 32 keys page up to the last)

CATone V2.9
- Up to 64 BISS/Fixed CW keys (pressing Radio Button will extend key selection to 64 keys - toggle function)
- Added name for some known BISS/CW Provider (@Cyrus prayer release) 

CATone V2.8
- Fixed DCW and BISS key handling press Radio key on RCU or P+ P- to switch between different CA.
  Each stored key is 10 bytes format compatible with DSR v5.4 ( SID + PMT * KEY without parity bytes)
- Removed backward compatibility with old keybin files (Hot7.4 onward) 
- removed possibility to add fixed DCW into PMCT as it is now handled in bin file. 

CATone V2.7
- 16 Cryptoworks providers added subtracting 48 bytes to keyspace.
- Pressing Epg in Ram editor allows to select 4 working modes:
	- both original Nagra - 5 providers and new Nagra - 17 providers (N-5  N-17)
	- Cryptowrks  (CR + N-5  CR + N-17)
- Cryptoworks CA system is directly accessed by grey key "mute"
- P+ and P- may now be used to cyclically switch Coding system
- Corrected edit mode in PMCT. Pressing OK allows to add a new raw to PMCT ram only if it is not
  already present otherwise it will be modified.
- in ECM-DW submenu is now possible to check fixed DCW adding them to pmct ram 
	in this format: CA CA KEY KEY KEY KEY KEY KEY KEY KEY
	example
									06 08  11  22  33  44  55  66  77  88
	to place 16 bytes simply edit twice.								

CATone V2.6
- Changed Nagra Irdeto Mode Detection.
 	One byte at offset is 0x208 is checked. 
 	If it is equal to 0x05 (5) then Bin File will be read as a traditional Bin File (N-5)
 	If it is 0x011 (17) then Bin is read as new type.(N-17)
 	All other values are forced to be 0x11 (N-17).
 	Pressing EPG allows to override automatic detection and to manually select desired mode  

CATone V2.5
- Fixed Bugs in nagra providers detection
- Added Enhanced Nagra Irdeto Mode to host 17 nagra providers (HOT>=7.1). 
  To select this mode press EPG while Ram Editor is ON. This setting is stored and automatically recalled.

CATone V2.4
- Not Public	

CATone V2.3
- Fixed small bugs
- Changed Teletext description in parser

CATone V2.2 
- Not Public

- 	Added Edit Mode in PMT parser. Just select blue tab and OK on the desired line, 
		and an item will be added at the end of PMCT
- 	Now it's possible to delete keys and providers. In ram editor just press three times ON/OFF (STDBY) button
  	on the desired item. A self-disappearing banner will confirm operation. 
  	Deleting a provider cause the deletion of all its keys.
- 	Adjusted some minor bugs (hope not to have added further ones)
-   scrolling on LCD
.....


CATone V2.1

- Key Edit select CA system by rcu colors;
- in case current channel is decripted by emu the editor should start showing actual provider
	and key in use marked in red (in Irdeto,Beta it only shows 1st Iredto provider);
- Provider name for known providers is shown;
- Fully implemented CAT and PMT parser. 3 views available : compact, full, hex data;
- views and preferences are now stored:
	-> possible to use different color schemes for 
		 a-start menu, about and help
		 b-key editor
		 c-parser
		 d-ecm-dw
	-> preferred parser view is stored for both CAT and PMT (may be different)
	-> at each calling CATone starts recalling last stored views.
	-> CATone preferences (and other things :) ) are resetted when reloading complete setting list.


CATone is free. Nothing may be modified. Neither FW nor Strings. 
This readme should accompany any CATone distribution.

Enjoy.

SuD

CATone v 2.0

- Not Public 


CATone v 1.4

- Not Public 


CATone v 1.3 

- corrected additional bugs 
- fully implemented AU fields editing 



CATone v 1.2

- Not Public 



CATone v 1.1 

- Corrected some bugs; 
- resizing to easily fit in 16/9 screens 


CATone v 1.0 

IT is still not complete and to improve it. 
known issues: 
- Not possible to edit PPUA, HMK,PMK, etc etc. for AU (TO do but the only one needed is Irdeto cause others are not AU) 
- Not possible to edit Conax Keys (I think nobady will have patience to write 128 bytes by hands) 
- PMT parser is missing (on going) 
- Problems on 16/9 screens or some clipping while editing keys in some 4/3 (I have to compoct keys).


Thanks to ToH for their precious work, and to Humax-Zone.net for the support.


CATone is free. Nothing may be modified. Neither FW nor Strings. 
This readme should accompany any CATone distribution.

Sturm und Drang.

