1. IRD Status
   (1) System ID : 406
   (2) Loader Version : L4.06
   (3) Device Version : v5.2.71
   (4) Application Version : TF-NCPC 5.11.88/TF-NPC 5.11.88
   (5) Last Update : Jun 10 2005

2. Improvements of this version
   (1) Some TAP applications did not work at the last beta version. It is fixed.
   (2) Sometimes the $ mark disappeared while recording. It is fixed.
   (3) There was some descrambling problem when changing the service from FTA to CAS in the TP with high data rate.
       It is fixed.

3. Notice
   (1) You can enable the option of dual descramble in Main Menu -> Common Interface -> Descramble multiple services.
       In this case, you have to use only one CAM with dual descramble function.

===================================================================================================
1. IRD Status
   (1) System ID : 406
   (2) Loader Version : L4.06
   (3) Device Version : v5.2.69
   (4) Application Version : TF-NCPC 5.11.85/TF-NPC 5.11.85
   (5) Last Update : June 02 2005

2. Improvements of this version
   (1) The MP3 files with two ID3 headers can be playback from this version.
   (2) The Prev/Next keys can be used in the status of timeshift bar to move the playback position
       to the start of timeshift buffer or live picture.
       The Prev/Next mean the positioning keys of PIP sub-picture (|< or >|).
   (3) The current time will be shown in the "Timer Setting" menu.
   (4) There was no sound in case of MP3 playback with pin code window. It is fixed.
   (5) The service was not changed with V- key in case of the service count under 4 in EPG. It is fixed.
   (6) There was some cases that all the services were grayed in the service list while recording.
       It may be fixed :-)
   (7) The descrambling problem in the multifeed services is fixed.
   (8) Some new TAP functions are supported.
       Please refer to the new TAP document which will be avaialbe in several days.
   (9) The system hanged up when the EPG key was pressed in the file list while playback.
       It is fixed.
   (10) The system did not check the collision of recording reservation after changing the duration
        in the "End of Recording" window. It is fixed.
   (11) The subtitle was not erased in some cases. It is fixed.
   (12) The recording file with the recording time less than 1 minute will be deleted.
        Some previous firmwares had this problem.
   (13) The recording file name might be "***-2" even though there is no file of "***". It is fixed.
        Some previous firmwares had this problem.
   (14) Dual descrambling in PIP is supported with the dual descambling CAM such as some versions of Aston CAM.
   (15) You can set the second audio and subtitle language.
        These selections will be activated if there is no track for the first language.
   (16) There was some display problem in the file list in case of some special characters in the file name.
        It is fixed.
   (17) The system hanged up when pressing OK key in "Conditional Access" menu. (TF5500PVR only)
        It is fixed. The last firmware had this problem.
   (18) There were the problems of freezing sub-picture or diabling timeshift in case of exchanging main-picture and sub-picture
        which is the service of different TP from the main picture.
        It is fixed.
   (19) The system hanged up in case of a very long time of turbo mode in Altair. It is fixed.
   (20) The system hanged up in case of starting recording with "Enrty Information" window.It is fixed.
   (21) The packet data of new PID was omitted if the PID information was changed at the starting point of recording.
        It is fixed.
   (22) There were some cases that it is impossible to activate the copy function for the recorded file.
        If you tried to copy the file at this case, the 0 MB file was created.
        No file will be made from this version.

===================================================================================================
1. IRD Status
   (1) System ID : 406
   (2) Loader Version : L4.06
   (3) Device Version : v5.2.66
   (4) Application Version : TF-NCPC 5.11.55/TF-NPC 5.11.55
   (5) Last Update : Mar 24 2005

2. Improvements of this version
   (1) The recording problem in Hotbird 11.054H and 11.604H is fixed.
       But, the file with empty name from the previous beta version still cannot be deleted.
       We will release the temporary firmware only to delete these files within next weekend.
   (2) The timer setting with "Record Off" did not function correctly in case of changing the wakeup service.
       It is fixed.
   (3) Some german string is modified.
   (4) There were some problems in the extended EPG of the recording info window which is shown
       by pressing "rec" button while recording.
       They are partly fixed. A little(?) problem is still left.
   (5) The text splitting in the extended EPG window is enhanced at this version.
   (6) Some bugs in the TAP were fixed and some TAP functions were added.
       We will release new TAP document soon.

===================================================================================================
1. IRD Status
   (1) System ID : 406
   (2) Loader Version : L4.06
   (3) Device Version : v5.2.66
   (4) Application Version : TF-NCPC 5.11.52/TF-NPC 5.11.52
   (5) Last Update : Mar 18 2005

2. Improvements of this version
   (1) The system hangup problem in some extended EPG has been cleared.
   (2) If you press 'rec' button while recording, new window will be shown.
       It is for quick modification of recording options.
       You can pause the recording process temporarily in this window.
   (3) Some TAP functions are added.
       The new TAP document is avaliable in Topfield's homepage. Please refer to the revison history.
   (4) One more universal LNB type of 9750/10750 is added.
   (5) The teletext and subtitle had some problems in case of lots of data to be displayed.
       It is fixed.
   (6) The subtitle will be shown even at playback from pause.
   (7) The system will be faster in the service with big EPG data.
   (8) There was a problem of mixing up the PIP services while dual recording. It is fixed.
   (9) The dual recording problem for two services in the same transponder is fixed.
   (10) There was some problem in checking the available services while dual recording. It is fixed.
   (11) And, more than 10 minor bugs were fixed.

===================================================================================================
1. IRD status
   (1) System ID : 406
   (2) Loader Version : L4.06
   (3) Device Version : v5.2.63
   (4) Application Version : TF-NCPC 5.11.44/TF-NPC 5.11.44
   (5) Last Update : Feb 03 2005

2. Improvements of this version
   (1) The problem of RCU key reaction is fixed.
       It was the side effect of processing all the key inputs.
   (2) All the problem of "grayed out" service list are fixed.
   (3) The reserved recording file name in record menu was set to the reserved event name
       in the EPG. It is fixed.
   (4) The time information will be displayed even in timeshift while recording.
   (5) The file will not be cut if you exit from the "cut" prompt.
   (6) The event information in the recorded file will be selected from the 10% position of
       recorded file or 10 minutes point of recorded file to get the exact event information.
   (7) If the copy function and the delayed recording conflict due to the limitation of
       main IC, the copy function will be stopped with the mark of "Incompleted Copy" in the recorded file.
   (8) The recorded file with the very long name was not copied. It is fixed.
   (9) There was the problem of stopping descramble in case of waiting for user confirmation of recording stop.
       It is fixed. (only for CONAX in TF5500PVR)
   (10) Cryptoworks CAM will work without any problem.

===================================================================================================
1. IRD status
   (1) System ID : 406
   (2) Loader Version : L4.06
   (3) Device Version : v5.2.61
   (4) Application Version : TF-NCPC 5.11.39/TF-NPC 5.11.39
   (5) Last Update : Jan 13 2005

2. Improvements of this version
   (1) There was a bug of displaying the opposite time format in case of standby.
       The 12-hour time format is removed because nobody seems to like it:-)
   (2) There were some cases of "grayed out" service list while recording with PIP.
       It is fixed.
   (3) This version RE-supports automatic tuner selection when you reserve the delayed
       recording in EPG.

===================================================================================================
1. IRD status
   (1) System ID : 406
   (2) Loader Version : L4.06
   (3) Device Version : v5.2.61
   (4) Application Version : TF-NCPC 5.11.38/TF-NPC 5.11.38
   (5) Last Update : Jan 07 2005

2. Improvements of this version
   (1) The system was very slow in Mediahighway EPG services at the last beta version (Dec 06 2004).
       It is fixed at this version.
   (2) Some DiSEqC switches were not compatible with TF5000PVR.
       This problem is fixed.

===================================================================================================
1. IRD status
   (1) System ID : 406
   (2) Loader Version : L4.06
   (3) Device Version : v5.2.60
   (4) Application Version : TF-NCPC 5.11.33/TF-NPC 5.11.33
   (5) Last Update : Dec 07 2004

2. Improvements of this version
   (1) The last beta version (Dec 03) has a EPG problem in Mediahighway services.
       The extended EPG information is not displayed.
       It is fixed at this version.

===================================================================================================
1. IRD status -- Beta version
   (1) System ID : 406
   (2) Loader Version : L4.06
   (3) Device Version : v5.2.60
   (4) Application Version : TF-NCPC 5.11.32/TF-NPC 5.11.32
   (5) Last Update : Dec 03 2004

2. Improvements of this version
   (1) The last beta version (Nov 29) has a critical problem in the parental control.
       There was no way to input the pincode in case of the censorship block.
       It is fixed.

===================================================================================================
1. IRD status -- Beta version
   (1) System ID : 406
   (2) Loader Version : L4.06
   (3) Device Version : v5.2.60
   (4) Application Version : TF-NCPC 5.11.31/TF-NPC 5.11.31
   (5) Last Update : Nov 29 2004

2. Improvements of this version
   (1) There were some cases of missing the delayed recording. It is fixed.
   (2) The time offset problem was fixed in winter time of MediaHighway EPG.
   (3) The DVB subtitle was not recorded. It is fixed.

===================================================================================================
1. IRD status -- Beta version
   (1) System ID : 406
   (2) Loader Ver. : L4.06
   (3) Device Ver. : v5.2.56
   (4) Application Ver. : TF-NCPC 5.11.27/TF-NPC 5.11.27
   (5) Last Update : Oct 21 2004

2. Improvements of this version
   (1) The problem while factory setting is fixed.
   (2) Hang up in TAP is fixed.
   (3) Problem in delayed recording is fixed.
   (4) DiSEqC1.2, DiSEqC1.3(USALS) is fixed.
   (5) Timeshift Progress Bar problem while trick mode is fixed.
   (6) Timeshift/Recording in Multifeed service is fixed.
   (7) Some other small bugs are fixed.

===================================================================================================
1. IRD status -- Beta version
   (1) System ID : 406
   (2) Loader Version : L4.06
   (3) Device Version : v5.2.56
   (4) Application Version : TF-NPC 5.11.24
   (5) Last Update : Oct 15 2004

2. Improvements of this version
   (1) Finland Language is supported.
   (2) Time format can be selected. (12 hour format or 24 hour format)
   (3) EPG is upgraded.
   (4) Bug on 'Channel lock function' is fixed.
   (5) It will move to the service which will be recorded when the power is turned on
       by the delayed recording function.
   (6) Bug in 'Service Rename'function is fixed.
   (7) The other functions are fixed.

===================================================================================================
1. IRD status -- Beta version
   (1) System ID : 406
   (2) Loader Ver. : L4.06
   (3) Device Ver. : v5.2.55
   (4) Appl Version : TF-NCPC 5.11.11/TF-NPC 5.11.11
   (5) Last Update : Jul 27 2004

2. Improvements of this version
   (1) Canal EPG is modified
   (2) Modified to fully compatible to SCM Module(CAM)
   (3) Recording, Playback and Copying of CAS services are modified.
       Delayed Recording is modified.
   (4) If the duration while recording is set to 0, the PVR will record till the HDD is full.
   (5) Message will be displayed while booting if there is some link error in HDD and the PVR is correcting it.
   (6) Some TAP function is added. ( The TAP API will be released later.)
   (7) Closed Caption(for SkyperfectTV) is supported
   (8) The Progress bar will appear if FF or RW button is pressed more than 1 seconds.
       In this case, the progress bar will be disappeared after 1 second if you don¡¯t press any button.
   (9) The Progress bar will appear if F3 button is pressed.
       In this case, the progress bar will disappear after 1 second if you don¡¯t press any button.
   (10) The bug the services that have very long name were not recorded is fixed.
   (12) Teletext function is modified. (Although the Packet Sequence is not correct it runs.)
   (13) Delayed Recording modified in EPG will be displayed to Rt in EPG.
   (14) EPG is modified. (The display is not modified.)
   (15) Some small bugs are fixed.

===================================================================================================
1. IRD status
   (1) System ID : 406
   (2) Loader Version : L4.06
   (3) Device Version : v5.2.51
   (4) Application Version : TF-NPC 5.10.97 / TF-NCPC 5.10.97
   (5) Last Update : May 19 2004

2. Improvements of this version
   (1) GMT Collection item in Time Setting Menu is added.
       It can be used to avoid wrong time information from some TPs.
       - Normal : The GMT is gathered from all the TPs
       - CAS Only : The GMT is gathered from CAS services.
       - User select : The GMT is gathered from the TP that user selected.

===================================================================================================
1. IRD status of Apr 30 2004 version
   (1) System ID : 406
   (2) Loader Ver : L4.06
   (3) Device Ver : v5.2.50
   (4) Application Ver. : TF-NCPC / TF-NPC 5.10.94
   (5) Last Update : Apr 30 2004

2. Improvements of this version
   (1) The problem in Canal EPG (MediaHighway EPG) is fixed.
       Set the MediaHighway menu to 'ON' to use the MediaHighway EPG.
       You can find the MediaHighway menu in Sytem Setting menu.
       After setting the MediaHighway menu to 'ON', turn off the PVR and turn on again to use the EPG.
   (2) Reservation on EPG is modified.
       - Press REC(red) button to record it and modify the reservation.
       - The state will be changed as follows by pressing the REC button repeatedly.
       Delayed Recording ("R") -> Edit the parameters of reservation -> Cancel
       By this function, the start time and end time can be modified.
       It will be very useful when the start time or end time of the EPG is not correct.
       If you change the start time or end time the icon will be changed to "Rt".

       * The function of OK button is same as previous.
       Reserve Play ("P") -> Reserve Recording ("R") -> Cancel

   (3) Teletext subpage is supported.
   (4) The audio drop in 3645/H/28000 TP of satellite Yamal-102 is fixed.

===================================================================================================
1. IRD status of Mar 12 2004 version
   (1) System ID : 406
   (2) Loader Version : L4.06
   (3) Device Version : v5.2.46
   (4) Software Version : TF-NPC 5.10.71
   (5) Last Update : Mar 12 2004

2. Improvements of this version
   (1) The problem in service changing of Cryptoworks/ORF channel is fixed.
   (2) Skip of recording in some Russian channel is fixed.

===================================================================================================
1. IRD status of Feb 06 2004 version
   (1) System ID : 406
   (2) Loader Version : L4.06
   (3) Device Version : v5.2.43
   (4) Software Version : TF-NPC 5.10.62
   (5) Last Update : Feb 03 2004

2. Improvements of this version
   (1) The problem of Audio Dropout is fixed.
   (2) The background-screen was broken during MP3 Play and playback the channel supporting DVB-Subtitle.
       It is fixed.
   (3) Sometimes sound mode was set to Mono in playback. It is fixed.
   (4) The problem at recording file name is fixed.

===================================================================================================
1. IRD status of Dec 06 2003 version
   (1) System ID : 406
   (2) Device Version : v5.2.40
   (3) Application Version : TF-NPC 5.10.56
   (4) Last Update : Dec 05 2003

2. Improvements of this version
   (1) The problem of EPG is fixed
   (2) The output level of YUV is modified.
   (3) The CI Menu is improved.
   (4) The size of MP3 file is not limited.
   (5) Recording during can be set by 1 minute.
   (6) There was a problem in recorded file copy from PVR to PC in Astra(11837/27500/H).
       It is fixed.
   (7) The problem in cutting scrambled file is fixed.
   (8) The RF output was black and white in Super Video Mode. It is fixed.
   (9) The default setting in search menu is changed from Network Search On to Network Search Off
   (10) "CAM initializing" message is displayed too much. It is modified.
   (11) Other some bugs are fixed.

===================================================================================================
1. IRD status
   (1) System ID : 406
   (2) Loader Version : L4.06
   (3) Device Version : v5.2.33
   (4) Application Version : TF-NPC 5.10.47
   (5) Last Update : Nov 06 2003

2. Improvements of this version
   (1) The Canal+ EPG is supported.
   (2) The problem in the large HDD is fixed.
   (3) The Subtile is modified.
   (3) Bookmarks for files in subfolder can be set.
   (4) The new bug that PVR can not descramble during recording at ver 5.10.44 is fixed.
   (5) The problem at reservation in EPG is fixed.

   The followings were improved in the last Beta software.

   (1) The CAM Initializing problem at a specific CAM is fixed.
   (2) DVB Subtitle is added.
   (3) The improper name at reservation by EPG is fixed.
   (3) Automatic Tuner selection by EPG reservation is added.
   (4) Timeshift is not stop while recording starts with the other.
   (5) PIP channel number was not updated. It is fixed.
   (6) Duplicate name for delayed recording is permitted from this version.
   (7) Multifeed problem is fixed.
   (8) Subtitle text was not deleted when the channel was changed. It is fixed.
   (9) Wrong favorite selection problem is fixed.
   (10)Hang up rarely while rewinding is fixed
   (11)File system of HDD is changed. (The old HDD is converted automatically by updating the firmware.)

===================================================================================================
1. IRD status of Aug 25 2003 version
   (1) System ID : 406
   (2) Device Version : v5.1.30
   (3) Application Version : TF-NPC 5.10.40
   (4) Last Update : Aug 25 2003

2. Improvements of this version
   (1) The command of DiSEqC 1.1 was not issued in case of service change with P+/P- keys.
       It is fixed.
   (2) The popup message while moving dish will be kept till channel locking.
   (3) The system halted when the prompt box of parental pincode shows.
       It is fixed.
   (4) The bootup time is much shortened, especially in case of many files in HDD.
   (5) You can select the satellite with 'Sat' key in service list.
   (6) There was a flickering problem in the copy function even with the normal speed.
       It is fixed.
   (7) The SPDIF audio will be muted when you execute 'Pause'.
   (8) The audio dropout in AC3 track is fixed.
   (9) The audio problem is much improved.
       - The dropout in ORF service is fixed.
       - There was a muting problem in some sound tracks at the services of Viasat.
         It is also fixed.
       - No audio in right channel at some services is fixed.
   (10) A scroll bar is added in the service list.
        You can estimate the current position.

===================================================================================================
1. IRD status of Jul 16 2003 version
   (1) System ID : 406
   (2) Device Version : v5.1.21
   (3) Application Version : TF-NPC 5.10.33
   (4) Last Update : Jul 16 2003

2. Improvements of this version
   (1) YUV mode in video output is available.
       Y/U/V signals will be out via the G/B/R pins of SCART connector.
   (2) DiSEqC 1.1 is available. Only switch 1/2 is supported.
   (3) No popup message was shown while moving dish with DiSEqC 1.2 or USALS.
       It is fixed.
   (4) A prompt window will be displayed in case of standby key while recording.
       If you don't close this window, the TF5000PVR will go to standby mode
       after finishing the record.
   (5) The PID window in advanced search mode was corrupted. It is fixed.
   (6) The information of free space in HDD will be accurate even though
       you move some folders to other folder.

===================================================================================================
1. IRD status of Jul 03 2003 version
   (1) System ID : 406
   (2) Device Version : v5.1.18
   (3) Application Version : TF-NPC 5.10.31
   (4) Last Update : Jul 03 2003

2. Improvements of this version
   (1) There was a problem in decoding AC3 at some AV receivers. It is fixed.
   (2) A folder can hold up to 4096 MP3 files.
   (3) It is possible to decode MP3 files with the broken header.
   (4) The functions for TAP are enhanced.
       We will release the sample TAP application using the upgraded functions next week.
       It is JPEG viewer which does the slide show while MP3 decoding or radio mode.

===================================================================================================
1. IRD status of Jun 16 2003 version
   (1) System ID : 406
   (2) Device Version : v5.1.16
   (3) Application Version : TF-NPC 5.10.27
   (4) Last Update : Jun 16 2003

2. Improvements of this version
   (1) All the MP3 files in a folder can be playback successively if you press '>' key
       with the cursor on that folder. RED key may be used to select the folder.
   (2) The repeat mode in MP3 is supported. The repeat mode will be toggled by WHITE key
       with the sequence of one song, all song and no repeat mode.
   (3) More distinctive display in the selection of MP3 or recorded files.
   (4) The infobox will show the information of MP3 file such as the singer, song name, bit rate,
       frequency, length and current position if they are available.
   (5) Some TAP applications could not work if they are in the sub-folder. It is fixed.
   (6) The TAP applications with TSR mode will have no problem from this version.

3. Notice
   (1) We got the report that the fast forward may cause the scrambled picture.
       We wonder that the CI CAM may have some limitations in descrambling the services with fast forward.
       According to the MPEG specifications on MP@ML, about 15 Mbps is the maximum bit rate
       for one video services.
       The normal bit rate of a TV service is 4~6 Mbps so 4x playback exceeds almost maximum bit rate.
       We cannot blame the CAM just because it cannot descramble the video over than the specifications.
       Furthermore, we also found some CAMs which hangs up in case of very high data rate.
       So, we recommend to copy with normal playback if you want to possess the important files in
       the clean(descrambed) format.

===================================================================================================
1. IRD status of Jun 04 2003 version
   (1) System ID : 406
   (2) Device Version : v5.1.15
   (3) Application Version : TF-NPC 5.10.23
   (4) Last Update : Jun 04 2003

2. Improvements of this version
   (1) The subtitle with teletext mode will be displayed without black bar.
   (2) The level of signal_quality_bar shows more actual state than the previous version.
   (3) There was a problem in the position of the current cursor at the multichannel EPG mode.
       It is fixed.
   (4) The EEPG will be saved while recording even though there is no EEPG information
       at the starting point of recording.
   (5) The copy will work without problem even if the recorded file has more than 2 hours length.
   (6) The information about the scramble/descramble in the recorded files is refined.
   (7) There was a problem in the backward playback in case of live picture in recording service.
       It is fixed.
   (8) The CAS service could not be decoded in the sub-picture while playback MP3 file.
       It is fixed.

===================================================================================================
1. IRD status of May 30 2003 version
   (1) System ID : 406
   (2) Device Version : v5.1.14
   (3) Application Version : TF-NPC 5.10.21
   (4) Last Update : May 30 2003

2. Improvements of this version
   (1) The screen will go black in radio mode after several minutes without user key operation.
       It's to avoid the damage of CRT screen in case that the same image is out for very long long time.
   (2) You can select any services for sub-picture while playback or MP3 decoding.
       There were some limitations in the previous firmware.
   (3) The subtitle with teletext mode will be displayed without black background.
   (4) The problem of file-cut is really fixed.
   (5) The acoustic noise from HDD is reduced while watching the live picture.
   (6) The problem of naming the repeated recordings are fixed.

===================================================================================================
1. IRD status of May 27 2003 version
   (1) System ID : 406
   (2) Device Version : v5.1.13
   (3) Application Version : TF-NPC 5.10.20
   (4) Last Update : May 27 2003

2. Improvements of this version
   (1) The new HDD could not be formatted. It is fixed. The system asks for user confirmation to format it.
   (2) The file which is recorded in time shifting mode will be shown in Altair from this version.
   (3) The transferred MPEG file from PC made the system failure if you try to playback. It is fixed.
   (4) The problem of file-cut is fixed.
   (5) There was a problem in mono sound mode. It is fixed.


