ZCAS to UCAS3.2 update file for MatrixCAM Reborn

Readme.txt			- You are reading this!
zcas2ucas.upd			- Update file for PCMCIA/serial board method
Uload_software_flash.hex 	- Flash memory for Funcard5 and Funcard6
Uload_software_flash_FUN7.hex	- Flash memory for Funcard7
zcas2ucas_512_x_x.hex		- EEPROM hex file for Funcard5
zcas2ucas_1024_x_x.hex		- EEPROM hex file for Funcard6
zcas2ucas_2048_x_x.hex		- EEPROM hex file for Funcard7

<IMPORTANT>

	After the upgrade to UCAS3.2, you need to leave the CAM in the receiver with live signal 
for 5-10 seconds.  This will activate its download subsystem.

