Humax ToH3.4 HoTplugged v11.5 - 2011-01-08
-- Version: A --
============================
- AustriaSat fix (cryptoworks) on 19.2E
	Important information for Humax-5400-users and File-Guys:
	As soon as EMU-decryption of ORF and/or AustriaSat will be over,
	you should delete (= value "00 00 00 ...") all Keys related to 
	ORF (Provider-ID "0D0540") and/or AustriaSat (Provider-ID "0D0510").
	This deletion will make sure that subscriber cards for ORF or 
	AustriaSat can work in an external CAM.

- Satellite Names (see drop-down list in the Humax-menu "Antenna Setting")
	have been revised and partly replaced by new ones

  new				old
  ---				---
  Astra 3 (23.5E)		Astra 3A,1E,1G (23.5E)
  Astra 4 (4.8E)		Sirius (4.8E)
  Atlantic Bird 1 (12.5W)	Atlantic Bird 2 (8W)

  For correct display of all firmware-embedded Satellite Names you
  should use the editor HNFSmart2.4fix2 (by Nostromo) and replace the old 
  file "satnames.ini" in the folder of HNFSmart2.4fix2 (usually in
  "C:\Programs\HumaxSmartSuite\HNFSmart") by the new file "satnames.ini" 
  that comes with current firmware ToH3.4HoT11.5 (see extra folder).
  (HNFSmart2.4fix2: http://www.humax-zone.net/index.php?page=5400_editors )

- new PMCT
  PMCT is available as:
    "PMCT_2011-01-08_ToH34HoT115.csv" (included in ToH3.4HoT11.5)
    "PMCT_2011-01-08_ToH34HoT115_only_for_A02-Card.csv" (use this one only if
	you have an Austrian A02-Card for Sky Germany in the internal slot)
  what has been done:
    Revision of EMU-related data
    Inclusion of new ProviderIDs and CAIDs
    Update of transponder tables for Quick Automatic Search
  Please NEVER delete transponder-data (Type-IDs "0050" to "0060") from 
    the PMCT if you distribute modified PMCTs on the internet! And you should 
    not distribute PMCTs that have simply been read from Humax and therefore 
    show no verbal information any more. Use the program "PMCTool", version
    0.1.4.0, if you want to modify the PMCT.
    (PMCTool 0.1.4.0: http://www.humax-zone.net/index.php?page=5400_tools )

*Some basic information on "CAID Preselect" and on "Cardblocker":
	Remember to use "CAID-Preselect = CARD+EMU" as standard.
	Choose "CARD+EMU+CS" only if you actually use Sharing-connections for 
		decryption or if the Humax 5400 shall work on Constant Control 
		Words (CCWs) for a while; additional CAMs with subscriber 
		cards for ORF/AustriaSat will not work on "CARD+EMU+CS".
	Choose "CARD+CS" only if you do not need the EMU at all: This option 
		is for decryption via Sharing and - maybe - subscriber card 
		in the internal	slot; additional CAMs with subscriber cards 
		for ORF/AustriaSat will not work on "CARD+CS".
	Select "Cardblocker = OFF" if you use a subscriber card 
		in the internal slot.
	Select "Cardblocker = ECM+EMM" if you use a mere dummy card
		in the internal slot.


Humax ToH3.4 HoTplugged v11.4 - 2010-03-05
-- Version: B --
============================
- bug fix v11.4 (Send DiSEqC twice for cascade)

Humax ToH3.4 HoTplugged v11.4 - 2010-03-01
-- Version: A --
============================
- KD Fix (nagra) on 23.5E

- new CAID Preselect Mode CARD-CS
  (CARD-CS-EMU not supported anymore)

- new CS-Protocol included: SSSP DSR
  works with DSR CardSharing Studio (thx to MAHDI)

  How to make your Humax work with DSR CS Studio 1.2:
    •	Set Sharing Protocol mode to SSSP DSR
    •	Set CAID Preselect to CARD+EMU+CS or CARD+CS
    •	Copy one of the plugins [example]  into your local folder Plugin 
	where the main program is located
    •	Configure your plugin with care
    •	Start program and select serial port (usually COM1) for connection
    •	Activate only one plugin!

  How to make your cccam work: see examples (-> DSR_CSStudio 1.2 -> Plugins)

    Hadu : Server=CCCam:MyServer.com:12000:0:MyUsername:MyPassword
    Acamd: cccamn:192.168.7.54:12000:0/0000/0000:username: password
    Flycccam (flydahli): C: xxx.xxx.xxx 12000 name pass
    WinCSC: edit wincsc.ini attached (working) or edit servers in 
	main plugin window

- Satellite Names (see drop-down list in the Humax-menu "Antenna Setting") 
	have been revised and mostly replaced by new ones (thx to Lombardo)

  new			old
  ---			---
  Astra 1		Astra 1
  Astra 2 & Eurob.1	Astra 2
  Hotbird		Hotbird
  EB & ES - 16.E	Eutelsat W2
  Eurobird 9		Eurobird 1
  Astra 3A,1E,1G	Astra 3A
  Eutelsat W3A		Telstar 11
  Turksat		Turksat 1C
  Hellas Sat		Intelsat 907
  Atlantic Bird 3	Intelsat 707
  Hispasat		Hispasat
  Thor & IS10-02	Thor 2,3
  Sirius		Sirius 2,3
  Badr			Arabsat 2A,3A,2D
  Amos			Amos 1
  Nilesat & AB4		Nilesat 101,102
  Atlantic Bird 2	Telecom 2D

  For correct display of the new firmware-embedded Satellite Names you
  should use the editor HNFSmart2.4fix2 (by Nostromo) and replace the old 
  file "satnames.ini" in the folder of HNFSmart2.4fix2 (usually in
  "C:\Programs\HumaxSmartSuite\HNFSmart") by the new file "satnames.ini" 
  that comes with current firmware ToH3.4HoT11.4 (see extra folder).
  (HNFSmart2.4fix2: http://www.humax-zone.net/index.php?page=5400_editors )

- brand-new PMCT (thx to Lombardo)
  PMCT_2010-03-04_ToH34HoT114.csv (included in 11.4)
  PMCT_2010-03-04_ToH34HoT114_only_for_SCT-Irdeto-Card.csv (use this one,
	if you have an original SCT Irdeto Card)  
  what has be done:
    Reworking of CAS Entries with respect to current EMU situation
    Reworking of priorities for CARD+EMU+CS and CARD+CS
    Inclusion of up-to-date CAID tables (VDR-Wiki)
    Update of transponder tables for Quick Automatic Search

- Default Send DiSEqC twice for cascade is OFF
  (Please be sure, that it's turned OFF if you don't need it)

- small bug fixes


Humax ToH3.4 HoTplugged v11.3 - 2010-02-06
-- Version: A --
============================
- VIA2.6 included

HoTplugged v11.1 - 2008-04-29
-- Version: A --
============================
- TV Gl*b* (13°E)  AU Fix


Humax ToH3.4 HoTplugged v11.0 - 2008-04-19
-- Version: A --
============================
- IRD2 PMKs now included in key.bin

	[HowTo]
	FreeX   IRD ProvID No 4 (IRD2 down!)
	SexView IRD ProvID No 5
	LA7	IRD ProvID No 6

	for AU you need: 

	Plain Mode:
	ProvID
	PMK0 stored in Key 0C/0D	
	PMK1 stored in Key 0E/0F

	crypted Mode:
	ProvId must be 000000	
	crypted ProvID is stored in Key 0A  
	crypted PMK0 is stored in Key 0C/0D	
	crypted PMK1 is stored in Key 0E/0F
	[/HowTo]

	for SexView include the following keys on IRD ProvID No 5
	ProvId must be 000000	
	0A: 9A9710B669C68128 
	0C: DFE674F4867E83A1 
	0D: A30C02595880CCB3
	0E: 4973A94D01179DB0 
	0F: 71F3D8943CA5757B


Humax ToH3.4 HoTplugged v10.9 - 2008-04-10
-- Version: A --
============================
- Sex View AU Fix


Humax ToH3.4 HoTplugged v10.8 - 2008-04-06
-- Version: A --
============================
- Sex View AU Fix


HoTplugged v10.7 - 2008-03-28
-- Version: A --
============================
- Polsat AU Fix 
- DigiTV AU Fix 
- TV Gl*b* (13°E)  AU

It is recommended to upload ToH3.4 HoTplugged v10.6b befor!


Humax ToH3.4 HoTplugged v10.6 - 2008-03-19
-- Version: B --
============================
- Fixed problem with x1.37 loaders (2nd try)


Humax ToH3.4 HoTplugged v10.6 - 2008-03-19
-- Version: A --
============================
- Sex View AU
- Fixed problem with x1.37 loaders

Humax ToH3.4 HoTplugged v10.5 - 2008-03-17
-- Version: A --
============================
- Free X AU
- LA7 AU


Humax ToH3.4 HoTplugged v10.4 - 2008-03-08
-- Version: A --
============================
- Nagra Fix 


Humax ToH3.4 HoTplugged v10.3 - 2008-03-05
-- Version: A --
============================
- PW Direkt Fix 
- TPS AU Fix 
- Polsat AU Fix 
- DigiTV AU Fix 

Humax ToH3.4 HoTplugged v10.2 - 2008-02-04
-- Version: A --
============================
- TPS AU Fix 

Humax ToH3.4 HoTplugged v10.1 - 2008-01-25
-- Version: A --
============================
- Polsat AU Fix 
- DigiTV AU Fix
- PW AU on Betacrypt (1702)


HoTplugged v10.0 - 2008-01-17
-- Version: A --
============================
- Polsat AU Fix
- small Fixes


HoTplugged v9.9 - 2008-01-05
-- Version: A --
============================
- PW AU Fix
- new Config Option Nagra2 AU
  o AUTO (Default) = AU only if necessary (Expired Keys)
  o ON = AU always 
  o OFF = AU disabled
 

don’t need to be converted for Humax 5400Z Plus!


HoTplugged v9.8 - 2007-12-20
-- Version: A --
============================
- PW Direkt/BlueMovie Fix 

HoTplugged v9.7 - 2007-12-05
-- Version: B --
============================
- PW AU Freeze Fix 

HoTplugged v9.7 - 2007-12-04
-- Version: A --
============================
- PW AU Fix 

Humax ToH3.4 HoTplugged v9.6 - 2007-11-21
-- Version: A --
============================
- Polsat AU Fix 
- TPS GMT Fix (summer/winter)
- D+ AU Fix
  Please notice that D+ AU is very processor intensive,
  therefore the Humax freeze during AU. AU need up to 
  5 Minutes. You must turn off and on to get AU.


Humax ToH3.4 HoTplugged v9.5 - 2007-09-09
-- Version: B --
============================
- Polsat AU Fix 
- biss detection fix for L1.37

Humax ToH3.4 HoTplugged v9.5 - 2007-09-07
-- Version: A --
============================
- Polsat AU 
(many THX to Mahdi)

Humax ToH3.4 HoTplugged v9.4 - 2007-09-05
-- Version: A --
============================
- Pixelerror Fix
- new structure for biss 
  frequency (Tolerance +/- 6) + SID (last Byte) + PMT (last byte) + key
  compatibel to SAMSUNG
- EMU moved to Module 4
- ORF Nagra Support
- Localia (30°W) Nagra Support (not tested)
- DigiTV AU

Humax ToH3.4 HoTplugged v9.3 - 2007-08-27
-- Version: A --
============================
- TV CABO AU Fix
- D+ AU Fix
- DigiTV Fix


Humax ToH3.4 HoTplugged v9.2 - 2007-08-19
-- Version: A --
============================
- TV CABO AU 
  please remove CAM while updating

Humax ToH3.4 HoTplugged v9.1 - 2007-08-13
-- Version: A --
============================
- D+ AU 
  please remove CAM while updating

Humax ToH3.4 HoTplugged v9.0 - 2007-08-12
-- Version: B --
============================
- PW AU fixed and enabled 

Humax ToH3.4 HoTplugged v9.0 - 2007-08-12
-- Version: A --
============================
- PW AU disabled  


Humax ToH3.4 HoTplugged v8.9 - 2007-08-11
-- Version: A --
============================
- Buli BugFix  


Humax ToH3.4 HoTplugged v8.8 - 2007-08-07
-- Version: A --
============================
- Showtime 7°W AU  
  (many THX to Mahdi, HNAGA and G++)


Humax ToH3.4 HoTplugged v8.7 - 2007-08-01
-- Version: B --
============================
- CAM FiX for TPS 

Humax ToH3.4 HoTplugged v8.7 - 2007-07-30
-- Version: A --
============================
- TPS AU on 10873 V (France4, France5)
  wait about 15 sec.
  tps.hdf disabled (no longer needed)
  (many THX to Mahdi).


Humax ToH3.4 HoTplugged v8.6 - 2007-07-23
-- Version: A --
============================
- TPS Fix (no AU yet)

 You just need to make a tps.hdf out of keyset.bin
 from TPS_Files_pack and load it into the Humax
 (on a daily basis). The first time you switch to
 TPS after startup, it will take some seconds to
 build the st20-Emualtor. Be sure that the time
 is set to GMT +2 (Central-Europe). 
 (many THX to Mahdi).

- Catone fix 3.2 included 

- Polsat key0/1 fix

- new bugs :)

thx also to Lombardo for the helpful bug list
	

Humax ToH3.4 HoTplugged v8.5 - 2007-07-16 
-- Version: A --
============================
- CAM-Support on CARD-EMU Mode

Humax ToH3.4 HoTplugged v8.4 - 2007-07-11 
-- Version: A --
============================
- Progress Bar on EPG info Panel

Humax ToH3.4 HoTplugged v8.3 - 2007-06-27 
-- Version: A --
============================
- Audioselection  fix

P.S.
forgotten: thx for G++ for the Turner RSA ;)

HoTplugged v8.2 - 2007-06-26 
-- Version: B --
============================
K*b*l Deutschland fixed
Absat (tps.bin) fixed

Humax ToH3.4 HoTplugged v8.2 - 2007-06-23 
-- Version: A --
============================
- Irdeto Card fix
- PMCT included (Transponder Update)


Humax ToH3.4 HoTplugged v8.1 - 2007-06-21 
-- Version: D --
============================
- VH1 & MTV Esp fix

Humax ToH3.4 HoTplugged v8.1 - 2007-06-20 
-- Version: C --
============================
- Tu*rner, S*yL*nk, K*b*l Deutschland included
- HSIC fixed

HoTplugged v8.1 - 2007-06-16 
-- Version: B --
============================
- D+ AU failed, disabled

HoTplugged v8.1 - 2007-06-16 
-- Version: A --
============================
- MECM60


(no PMCT included)
Humax ToH3.4 HoTplugged v8.0 - 2007-02-12 
-- Version: A --
============================
- D+ AU
- PW AU 

(no PMCT included)


Humax ToH3.4 HoTplugged v7.9 - 2007-01-02 
-- Version: A --
============================
- TP$ Fix 

(no PMCT included)

Humax ToH3.4 HoTplugged v7.8 - 2006-12-24 
-- Version: A --
============================
- TP$ Fix 

TP$.BIN can be loaded via hdfbin-3-006000.raw
(that raw can't be bigger then 0x9F00 bytes!)
time must be set correct (GMT) to get right TP$-key 


(no PMCT included)

Humax ToH3.4 HoTplugged v7.7 - 2006-12-01 
-- Version: A --
============================
- Cryptowork Fix 
- new structure for biss 

exp: Rai Asia ON HOTBIRD
SID = 2136
PMT = 0100
PCR = 00C8
key = 1122334455667788
SID + PMT last byte + PCR last byte + key
213600C81122334455667788

(no PMCT included)

Humax ToH3.4 HoTplugged v7.6 - 2006-09-09 
-- Version: B --
============================
- AES TPS Autoroll

Humax ToH3.4 HoTplugged v7.5 - 2006-05-26 
-- Version: A --
============================
- CW RSA Fix

Please Note:

When Using DSR 9500 EMU, Set "Humax Def", and Verify
from Box to "ON" in "?-context", always zap to a FTA-Channel
first or remove Card.

Please use Card+EMU (in TOH-Config) if you are not using CW-Sharing !
Please set Card Blocker to ECM+EMM if using a Dummy-Card !



Humax ToH3.4 HoTplugged v7.4 - 2006-05-24 
-- Version: A --
============================
- adapted to DSR 9500 EMU Ed54_CW.exe:
	Cryptoworks/BISS/fix CW/ loaded from key.bin
- DD Radio Fix

! old key.bins are not supported anymore

Humax ToH3.4 HoTplugged v7.3 - 2006-05-09 
-- Version: A --
============================
- CW included:

	EasyTV		ok

Humax ToH3.4 HoTplugged v7.2 - 2006-05-08 
-- Version: B --
============================
- CW freezing Fix


Humax ToH3.4 HoTplugged v7.2 - 2006-05-07 
-- Version: A --
============================
- CW included:

	DMC15°W		not tested
	JSTV		ok
	Kingstone	not tested
	Digiturk	nok
	Xtramusic	ok
	Turner		not tested
	Czech Link	not tested
	British Telecom	not tested
	Slovak Link	not tested


Humax ToH3.3 HoTplugged v7.0 - 2006-03-16 
-- Version: A --
============================
- N2 keys via key.bin

modify N2-RSA by keybin (NAGRA, PROVID):

   ecmMod[0x40]	 	= key 0 - 7
   ecmIkey[0x10] 	= key 8 - 9
   ecmIkey9x[0x10]	= key 0xA - 0xB
   ecmVkey[0x10]	= key 0xC - 0XD



Please: We need from the developer of Samy_Humy_Edit 
and/or DSR 9500 EMU Ed a new program version with more then
5 NAGRA-Provider. (20 would be great!) Please contact us on 
http://www.toh.humax-zone.tv/board/

We can't enlarge the number of providers in emu until we have
a new version of editor. :-/
Please we don't want release emu-versions with build-in keys in the
future. So this is very important to get a new keyedit-version !!!


Humax ToH3.3 HoTplugged v6.9 - 2006-03-12 
-- Version: A --
============================
- N2 Globecast added
- N2 Polsat added


Humax ToH3.3 HoTplugged v6.8 - 2006-02-14 
-- Version: A --
============================
- Bugfixes


Humax ToH3.3 HoTplugged v6.7 - 2006-02-03 
-- Version: A --
============================
- N2 TV CABO added



Humax ToH3.3 HoTplugged v6.6 - 2006-01-24 
-- Version: A --
============================
- D+ Fix 


Humax ToH3.3 HoTplugged v6.5 - 2006-01-09 
-- Version: B/C --
============================
- PMCT adjusted 
- bugfixes


Humax ToH3.3 HoTplugged v6.5 - 2006-01-04 
-- Version: A --
============================
- D+ Fix


Humax ToH3.3 HoTplugged v6.4 - 2005-12-24 
-- Version: A --
============================
- SSSP-Mode (gbox)

Humax ToH3.3 HoTplugged v6.1 - 2005-11-27 
-- Version: A --
============================


Humax ToH3.3 HoTplugged v6.2 - 2005-12-04 
-- Version: A --
============================
- Nagra AU disabled
- MTV-CW's


Humax ToH3.3 HoTplugged v6.1 - 2005-11-27 
-- Version: A --
============================
- Card Blocker included
  Use Option ECM/EMM for Dummy-Cards (recommended)
- Portal Fix
- some Bug-Fixes


Humax ToH3.3 HoTplugged v6.0 - 2005-11-20 
-- Version: A --
============================
- AES-Fix (Key 3 and 0x13)
- constant CW can be stored by 2 entries via PMCT like
  IDENT VPID CAS nnnn nnnn nnnn nnnn 0000 (=CW even)
  IDENT VPID CAS nnnn nnnn nnnn nnnn 0000 (=CW Odd)
  (untested)

Humax ToH3.3 HoTplugged v5.9 - 2005-10-23 
-- Version: A --
============================
- Cabo-AU Fix (Key0+1 OK - Key2+3 NOK)
- BISS included (Discovery dosn't work - don't know why)
  use PMCT to modify CWs
  IDENT VPID 2600 nnnn nnnn nnnn nnnn 0000
- EPG/PMCT-Menu use white Button to insert line instantly
- included CAToneV23-Parser
- AES-Key now on Key 3 and 0x13

thx to scriptors and GioppyGio 


Humax HoTplugged v5.8 - 03.09.2005 
-- Version: D+ is back :-) --
============================
- D+ MTV ESP Astra Fix
- DISH Network 61.5°W (ID 0101 - not tested) 


Humax ToH3.3 HoTplugged v5.7 - 27.08.2005 
-- Version: D+ is back :-) --
============================
- D+ Fix (maybe not for long time)

special thanks to:
humax hdl-Team for the code
st20tp2 for support & some pseudo C porting
siko-SK for firmwares rom & ramdump
remote, Nightshad & all people that help humax to extract algo...


Humax ToH3.3 HoTplugged v5.6 - 20.08.2008 
-- Version: Benedikt XVI  --
============================
( 20.08.2008 PMCT Bug-Fix because MCM)
 - MTV/VH1 on Astra Hack 
  (006A without Nano 5105)


Humax ToH3.3 HoTplugged v5.5 B
==============================
- Mediapark Fix

Humax ToH3.3 HoTplugged v5.5
============================
- PW Portal Fix (by Padawan)
- Nagra optimization
- Spice Fix


Humax ToH3.3 HoTplugged v5.4
============================
not released  



Humax ToH3.3 HoTplugged v5.3
============================
- Cabo Fix
- Irdeto Card-Fix


Humax ToH3.3 HoTplugged v5.2
============================

- ORF fix when PW-Card is used
- PK0 AU (Nagra) on Key2+3 (wait some minutes)
- tps crypt optimized
- version 2.1 of CATONE Conditional Access Tool included (thx to that team)

thx also to Humax & D-Mon



HoT



CATone V3.2


file CRC: 2AF7FC9B
file MD5: 832e89cf7a5e62fbb77bb316c0aa511f

History and changes

CATone V3.2
- Crytoworks provider name list updated
- Nagra current keyset bugfix

CATone V3.0
- Unlimited Number of BISS/Fixed CW Keys (up to key bin size!) 
  (multiple pressing Radio Button will show additinal 32 keys page 
  up to the last)

CATone V2.9
- Up to 64 BISS/Fixed CW keys (pressing Radio Button will extend 
  	key selection to 64 keys - toggle function)
- Added name for some known BISS/CW Provider (@Cyrus prayer release) 

CATone V2.8
- Fixed DCW and BISS key handling press Radio key on RCU or P+ P- to switch 
	between different CA.
  Each stored key is 10 bytes format compatible with DSR v5.4 
	( SID + PMT * KEY without parity bytes)
- Removed backward compatibility with old keybin files (Hot7.4 onward) 
- removed possibility to add fixed DCW into PMCT as it is now handled 
	in bin file. 

CATone V2.7
- 16 Cryptoworks providers added subtracting 48 bytes to keyspace.
- Pressing Epg in Ram editor allows to select 4 working modes:
	- both original Nagra - 5 providers and new Nagra - 17 providers 
		(N-5  N-17)
	- Cryptowrks  (CR + N-5  CR + N-17)
- Cryptoworks CA system is directly accessed by grey key "mute"
- P+ and P- may now be used to cyclically switch Coding system
- Corrected edit mode in PMCT. Pressing OK allows to add a new raw to 
	PMCT ram only if it is not already present 
	otherwise it will be modified.
- in ECM-DW submenu is now possible to check fixed DCW adding them to 
	pmct ram in this format: CA CA KEY KEY KEY KEY KEY KEY KEY KEY
	example
		06 08  11  22  33  44  55  66  77  88
	to place 16 bytes simply edit twice.								

CATone V2.6
- Changed Nagra Irdeto Mode Detection.
 	One byte at offset is 0x208 is checked. 
 	If it is equal to 0x05 (5) then Bin File will be read as 
		a traditional Bin File (N-5)
 	If it is 0x011 (17) then Bin is read as new type.(N-17)
 	All other values are forced to be 0x11 (N-17).
 	Pressing EPG allows to override automatic detection and to manually 
		select desired mode  

CATone V2.5
- Fixed Bugs in nagra providers detection
- Added Enhanced Nagra Irdeto Mode to host 17 nagra providers (HOT>=7.1). 
  To select this mode press EPG while Ram Editor is ON. This setting is 
  stored and automatically recalled.

CATone V2.4
- Not Public	

CATone V2.3
- Fixed small bugs
- Changed Teletext description in parser

CATone V2.2 
- Not Public

- 	Added Edit Mode in PMT parser. Just select blue tab and OK on 
		the desired line, and an item will be added at the end of PMCT
- 	Now it's possible to delete keys and providers. In ram editor just 
	press three times ON/OFF (STDBY) button on the desired item. 
	A self-disappearing banner will confirm operation. 
  	Deleting a provider cause the deletion of all its keys.
- 	Adjusted some minor bugs (hope not to have added further ones)
-   	scrolling on LCD
.....


CATone V2.1

- Key Edit select CA system by rcu colors;
- in case current channel is decripted by emu the editor should start showing 
	actual provider
	and key in use marked in red (in Irdeto,Beta it only shows 1st Irdeto 
	provider);
- Provider name for known providers is shown;
- Fully implemented CAT and PMT parser. 
  3 views available : compact, full, hex data;
- views and preferences are now stored:
	-> possible to use different color schemes for 
		 a-start menu, about and help
		 b-key editor
		 c-parser
		 d-ecm-dw
	-> preferred parser view is stored for both CAT and PMT 
	   (may be different)
	-> at each calling CATone starts recalling last stored views.
	-> CATone preferences (and other things :) ) are resetted when 
	   reloading complete setting list.


CATone is free. Nothing may be modified. Neither FW nor Strings. 
This readme should accompany any CATone distribution.

Enjoy.

SuD

CATone v 2.0

- Not Public 


CATone v 1.4

- Not Public 


CATone v 1.3 

- corrected additional bugs 
- fully implemented AU fields editing 



CATone v 1.2

- Not Public 



CATone v 1.1 

- Corrected some bugs; 
- resizing to easily fit in 16/9 screens 


CATone v 1.0 

IT is still not complete and to improve it. 
known issues: 
- Not possible to edit PPUA, HMK,PMK, etc etc. for AU (TO do but the only one 
  needed is Irdeto cause others are not AU) 
- Not possible to edit Conax Keys (I think nobady will have patience 
  to write 128 bytes by hands) 
- PMT parser is missing (on going) 
- Problems on 16/9 screens or some clipping while editing keys in some 4/3 
  (I have to compoct keys).


Thanks to ToH for their precious work, and to Humax-Zone.net for the support.


CATone is free. Nothing may be modified. Neither FW nor Strings. 
This readme should accompany any CATone distribution.

Sturm und Drang.

