# oscam.conf generated automatically by Streamboard OSCAM 1.20_svn SVN r11682
# Read more: https://svn.streamboard.tv/oscam/trunk/Distribution/doc/txt/oscam.conf.txt
[global]
logfile                       = /tmp/oscam.log
preferlocalcards              = 2

[cs378x]
port                          = 9001
suppresscmd08                 = 1

[dvbapi]
enabled                       = 1
au                            = 1
pmt_mode                      = 4
request_mode                  = 1
user                          = dvbapiau
read_sdt                      = 2
write_sdt_prov                = 1
boxtype                       = pc-nodmx

[webif]
httpport                      = 8888
httpuser                      = oscam
httppwd                       = WACHTWOORD
httphideidleclients           = 0
httpallowed                   = 127.0.0.1,192.168.0.0-192.168.255.255,192.168.1.0-192.168.255.255
aulow                         = 120
hideclient_to                 = 15

# oscam.user generated automatically by Streamboard OSCAM 1.20_svn SVN r11682
# Read more: https://svn.streamboard.tv/oscam/trunk/Distribution/doc/txt/oscam.user.txt

[account]
user                          = dvbapiau
caid                          = 0604
au                            = 1
group                         = 1

# oscam.server generated automatically by Streamboard OSCAM 1.20_svn SVN r11716
# Read more: https://svn.streamboard.tv/oscam/trunk/Distribution/doc/txt/oscam.server.txt

[reader]
label                         = ZiggoKaart
description                   = ZiggoKaart
protocol                      = smargo
device                        = /dev/ttyUSB0
autospeed                     = 0
caid                          = 0604
boxkey                        = 1122334455667788
rsakey                        = 3C8633AAC0D367533DEC7BB2EEEDEB8CA3ADA52E58B99BB34672783277A1DAAC3B6106AD0909774E031B2A6E30195B437683AD0FC599B87D08CEA47BE1B6C76A
detect                        = cd
mhz                           = 450
cardmhz                       = 2700
group                         = 1
emmcache                      = 1,3,2,0
cccreshare                    = 0

[reader]
label                         = upper_card
enable                        = 0
protocol                      = smargo
device                        = /dev/ttyUSB0
detect                        = cd
mhz                           = 450
cardmhz                       = 2700
group                         = 1
emmcache                      = 1,3,15,0
ratelimitecm                  = 4
ecmunique                     = 1
ratelimittime                 = 10000
srvidholdtime                 = 2000
cooldown                      = 30,600

[reader]
label                         = emulator
enable                        = 0
protocol                      = unknown
device                        = emulator
disablecrccws_only_for        = 0E00:000000
caid                          = 0500,0604,0D00,0E00,1010,1801,2600,2602,2610
detect                        = cd
ident                         = 0500:020A00,021110;0604:000000;0D00:0000C0;0E00:000000;1010:000000;1801:000000,001101,002111,007301;2600:000000;2602:000000;2610:000000
group                         = 2
emmcache                      = 2,1,2,1

2023/06/26 19:09:20  19ACE38 r   (reader) ZiggoKaart [smargo] Buffers readed  0 bytes total time_us 75147
2023/06/26 19:09:20  19ACE38 r   (reader) ZiggoKaart [smargo] Reader initialized (device=/dev/ttyUSB0, detect=cd, pll max=27.00 MHz, wanted mhz=4.50 MHz)
2023/06/26 19:09:20  19ACE38 r   (reader) ZiggoKaart [smargo] Reader sci internal, detected box type: generic
2023/06/26 19:09:20  19ACE38 r   (reader) ZiggoKaart [smargo] card detected
2023/06/26 19:09:28  19ACE38 r   (reader) ZiggoKaart [smargo] ATR: 3B 9F 21 0E 49 52 44 45 54 4F 20 41 43 53 20 56 35 2E 38 95 
2023/06/26 19:09:28  19ACE38 r   (reader) ZiggoKaart [smargo] Init card protocol T14, FI=2, F=558, D=1, N=0
2023/06/26 19:09:28  19ACE38 r   (reader) ZiggoKaart [smargo] Calculated work ETU is 124.00 us reader mhz = 450
2023/06/26 19:09:29  19ACE38 r   (reader) ZiggoKaart [smargo] ATR Fsmax is 6 MHz, clocking card to wanted user cardspeed off 4.50 MHz (specified in reader->mhz)
2023/06/26 19:09:30  19ACE38 r   (reader) ZiggoKaart [smargo] detect irdeto card
2023/06/26 19:09:30  19ACE38 r   (reader) ZiggoKaart [smargo] Irdeto SC 58 version 21 revision 1, patch level e
2023/06/26 19:09:30  19ACE38 r   (reader) ZiggoKaart [smargo] caid: 0604, acs: 0.05, country code: NLD
2023/06/26 19:09:30  19ACE38 r   (reader) ZiggoKaart [smargo] providers: 4, ascii serial: ##########, hex serial: ######, hex base: ##
2023/06/26 19:09:33  19ACE38 r   (reader) ZiggoKaart [smargo] WARNING: For Irdeto cards you will have to set 'cardmhz= 600' in oscam.server
2023/06/26 19:09:33  19ACE38 r   (reader) ZiggoKaart [smargo] active providers: 4 (0c54f1,ffffff,ffffff,ffffff)
2023/06/26 19:09:33  19ACE38 r   (reader) ZiggoKaart [smargo] found card system irdeto
2023/06/26 19:09:33  19ACE38 r   (reader) ZiggoKaart [irdeto] THIS WAS A SUCCESSFUL START ATTEMPT No  1 out of max alloted of 1
2023/06/26 19:09:33  19ACE38 r   (reader) ZiggoKaart [irdeto] entitlements for provider: 1, id: 0C54F1
2023/06/26 19:09:33  19ACE38 r   (reader) ZiggoKaart [irdeto] chid: 7FFE, date: 2017/06/12 - 2017/07/12
2023/06/26 19:09:33  19ACE38 r   (reader) ZiggoKaart [irdeto] chid: FFE0, date: 2023/06/24 - 2023/07/25
2023/06/26 19:09:33  19ACE38 r   (reader) ZiggoKaart [irdeto] chid: 000B, date: 2023/06/24 - 2024/01/11
2023/06/26 19:09:33  19ACE38 r   (reader) ZiggoKaart [irdeto] chid: 0384, date: 2023/06/24 - 2024/01/10
2023/06/26 19:09:33  19ACE38 r   (reader) ZiggoKaart [irdeto] chid: FFD8, date: 2023/06/24 - 2024/01/10
2023/06/26 19:09:33  19ACE38 r   (reader) ZiggoKaart [irdeto] chid: 7FFD, date: 2023/06/24 - 2023/07/04
2023/06/26 19:09:40  19ACE38 r   (reader) ZiggoKaart [irdeto] ready for requests
2023/06/26 19:09:41        0 s     (main) init for all local cards done
2023/06/26 19:09:41        0 s (emmcache) loaded 12 emmcache records from /tmp/.oscam/oscam.emmcache in 0 ms
2023/06/26 19:09:41        0 s (emmcache) loaded 12 emmstat records from /tmp/.oscam/oscam.emmstat in 0 ms
2023/06/26 19:09:41        0 s (anticasc) anti cascading disabled
2023/06/26 19:09:41  19A4380 c   (client) plain dvbapi-client granted (dvbapiau, au=auto (3 reader))
2023/06/26 19:09:41  19A4380 c   (dvbapi) dvbapi channelcache loaded from /usr/local/etc/oscam.ccache
2023/06/26 19:09:41  19A4380 c   (dvbapi) Using /tmp/camd.socket listen socket, API forced to DVBAPIv3 (0), userconfig boxtype: 12
2023/06/26 19:09:41        0   >> OSCam <<  cardserver log switched, version 1.20-unstable_svn, build r10630 (arm-linux-gnueabihf)
2023/06/26 19:09:43  19A4380 c   (dvbapi) Client connected: 'Tvheadend 4.3-1964~g637844055' (protocol version = 2)

Nadat ik RTL4 heb proberen te kijken:
2023/06/26 19:10:15  19A4380 c   (dvbapi) Demuxer 0 added new ecmpid 0 CAID: 1868 ECM_PID: 080E PROVID: 000000
2023/06/26 19:10:15  19A4380 c   (dvbapi) Demuxer 0 added new ecmpid 1 CAID: 1850 ECM_PID: 080D PROVID: 000000
2023/06/26 19:10:15  19A4380 c   (dvbapi) Demuxer 0 added new ecmpid 2 CAID: 1801 ECM_PID: 080C PROVID: 000000
2023/06/26 19:10:15  19A4380 c   (dvbapi) Demuxer 0 added new ecmpid 3 CAID: 0606 ECM_PID: 0804 PROVID: 000000
2023/06/26 19:10:15  19A4380 c   (dvbapi) Demuxer 0 added new ecmpid 4 CAID: 0604 ECM_PID: 0803 PROVID: 000000
2023/06/26 19:10:15  19A4380 c   (dvbapi) Demuxer 0 added new ecmpid 5 CAID: 0602 ECM_PID: 0802 PROVID: 000000
2023/06/26 19:10:15  19A4380 c   (dvbapi) Demuxer 0 found 6 ECMpids and 6 STREAMpids in PMT
2023/06/26 19:10:15  19A4380 c   (dvbapi) Demuxer 0 receiver wants to demux srvid 4C05 on adapter 0000 camask 0001 index 0000 pmtpid 07D0
2023/06/26 19:10:15  19A4380 c   (dvbapi) Demuxer 0 new program number: 4C05 (TV) [pmt_list_management 3]
2023/06/26 19:10:15  19A4380 c   (dvbapi) Demuxer 0 trying to descramble PID 4 CAID 0604 PROVID 000000 ECMPID 0803 ANY CHID PMTPID 07D0 VPID 07D1
2023/06/26 19:10:15  19A4380 c      (ecm) dvbapiau (0604&000000/000B/4C05/44:FE53D06FFB24B293A48DBA3EF3F8E3B8): found (204 ms) by ZiggoKaart - TV
2023/06/26 19:10:18  19A4380 c      (ecm) dvbapiau (0604&000000/000B/4C05/44:A78BF3E284DFB3BB68B5B3573FECB452): found (201 ms) by ZiggoKaart - TV
2023/06/26 19:10:36  19A4380 c   (dvbapi) Client connected: 'Tvheadend 4.3-1964~g637844055' (protocol version = 2)
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 added new ecmpid 0 CAID: 1868 ECM_PID: 080E PROVID: 000000
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 added new ecmpid 1 CAID: 1850 ECM_PID: 080D PROVID: 000000
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 added new ecmpid 2 CAID: 1801 ECM_PID: 080C PROVID: 000000
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 added new ecmpid 3 CAID: 0606 ECM_PID: 0804 PROVID: 000000
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 added new ecmpid 4 CAID: 0604 ECM_PID: 0803 PROVID: 000000
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 added new ecmpid 5 CAID: 0602 ECM_PID: 0802 PROVID: 000000
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 found 6 ECMpids and 6 STREAMpids in PMT
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 receiver wants to demux srvid 4C05 on adapter 0000 camask 0001 index 0000 pmtpid 07D0
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 new program number: 4C05 (TV) [pmt_list_management 3]
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 found channel in cache and matching prio -> start descrambling ecmpid 4 
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 trying to descramble PID 4 CAID 0604 PROVID 000000 ECMPID 0803 ANY CHID PMTPID 07D0 VPID 07D1
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 continue decoding of SRVID 4C05
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 added new ecmpid 0 CAID: 1868 ECM_PID: 080E PROVID: 000000
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 added new ecmpid 1 CAID: 1850 ECM_PID: 080D PROVID: 000000
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 added new ecmpid 2 CAID: 1801 ECM_PID: 080C PROVID: 000000
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 added new ecmpid 3 CAID: 0606 ECM_PID: 0804 PROVID: 000000
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 added new ecmpid 4 CAID: 0604 ECM_PID: 0803 PROVID: 000000
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 added new ecmpid 5 CAID: 0602 ECM_PID: 0802 PROVID: 000000
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 found 6 ECMpids and 6 STREAMpids in PMT
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 receiver wants to demux srvid 4C05 on adapter 0000 camask 0001 index 0000 pmtpid 07D0
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 new program number: 4C05 (TV) [pmt_list_management 3]
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 found channel in cache and matching prio -> start descrambling ecmpid 4 
2023/06/26 19:10:36  19A4380 c   (dvbapi) Demuxer 0 trying to descramble PID 4 CAID 0604 PROVID 000000 ECMPID 0803 ANY CHID PMTPID 07D0 VPID 07D1
2023/06/26 19:10:37  19A4380 c      (ecm) dvbapiau (0604&000000/000B/4C05/44:0D3B8556D4562D1562039449DD2E7AA6): found (200 ms) by ZiggoKaart - TV