RayhTec 11a firmware for Philips DSX607x (5 September 2009)


Changes:
CDW implemented with editor
GBOX Cardsharing improved
LNB indication in zap banner
Without card in decoder channel search is possible
Channeleditor (+B4) added with option CLEAR CHANNEL
EMU modified: TV Globo Nagra2 and 10722H Cryptoworks added


Remarks:
Take care of correct communication protocol in antenna configuration menu.
For AU Seca card in decoder is needed and Blocker OFF.


Features:
Menu languages: Dutch, English (Some French is implemented)
Seca2 and Seca 3 (Merlin) smartcard support. (Auto detection)
Cardemulator support:
SECA1/SECA2	   8 providers
VIACCESS 2.3	  20 providers
NAGRAVISION2	   5 providers
IRDETO1/BETACRYPT  9 providers
CRYPTOWORKS	  16 providers
CDW		  12 providers
No Conax implemented. Do not edit Conax keys in Cardemulator!

EMM Blocker: Blocks to smartcard and emulator (Not work for Merlin card)
Servicecard support
2000 channels and 254 transponders
DiSEqC 1.0 for switch
DiSEqC 1.2 for rotor
Automatic date/time adjustement at power up.
Remote key option (was used in the past for Funcard)
No interactivity
Symbolrate 	6071: 1…32 MS/s,
	 	6072: 12…30 MS/s
EPG according to MediaHigWay and DVB standard
Baudrate adjustable for Advanced Serial Communications (SAC):
	--> Baudrate adjustment in Menu, 4, 1, 9. Will be saved at standby.
	--> Choose +, B, 7 for set up SAC:
	    4 for MediaBox Communicator		
	    5 for sssp for GBOX or NewCamd server. Takes effect on channel switch.
	      Works simultanuously with card in decoder. 	
	--> Tested software: gbox225 and DSR9500Share


Remote key functions:
A	: Tune on channels which broadcasts radiochannels and press this key
B	: Picture on screen freezes
C	: No function
D	: Stream Grabber (Not all options are working anymore)
E	: zaplist
0	: Returns to previous watched channel
+	: Some channel information and access to servicemenu (B)
INFO	: Shows now/next information. When inputting keys this is character F
EPG	: Electronic Program Guide
	  MHW EPG : Working for Canal Digitaal, CanalSat, Cyfra and Sky Italia. D+ is not working
	  DVB EPG : All channels which are broadcasting EPG according to this standard.
	  	    (Premiere, German FTA, ORF, ABSat, SRG, for PolSat it is needed sometimes to press arrow left few times	
MENU	: Access to Main menu
PREF	: Switch on/off preference list

