Important advice for all users and appeal to the "Settings-Guys"
===============================================================

For ToH3.4HoT11.5 the firmware-embedded Satellite Names (see drop-down list 
in the Humax-menu "Antenna Setting") have been revised and partly replaced 
by new ones.

For correct display of all firmware-embedded Satellite Names you
should use the editor HNFSmart2.4fix2 (by Nostromo) and replace the old 
file "satnames.ini" in the folder of HNFSmart2.4fix2 (usually in
"C:\Programs\HumaxSmartSuite\HNFSmart") by the new file "satnames.ini" 
that comes with current firmware ToH3.4HoT11.5.

You can download the Settings-editor HNFSmart2.4fix2 from:
http://www.humax-zone.net/index.php?page=5400_editors



Unfortunately, there is no common agreement on which Antenna-/LNB-numbers 
are used for specific Satellite Names. Such an agreement would be desirable.

If you are going to distribute Settings-files on the internet, We would like 
to ask you that you use only firmware-embedded Satellite Names 
(not: user-defined Satellite Names) for the Antenna-/LNB-numbers 1 - 17 
and that you stick to the following relations:


  Antenna-/LNB-Number	firmware-embedded Satellite Name
  ----------------- 	--------------------------------
	1		"Astra 1" (19.2° East) 

	2		"Hotbird" (13° East)

	3		"Astra 4" (4.8° East)

	4		"Eutelsat W3A" (7° East)

	5		"Eurobird 9" (9° East)

	6		"EB & ES - 16°E" (= Eurobird 16A & Eutelsat Sesat 
					& Eutelsat W2M on 16° East)

	7		"Astra 3" (23.5° East)

	8		"Badr" (26° East)

	9		"Astra 2 & Eurob.1" (= Astra 2 on 28.2° East
					& Eurobird 1 on 28.5° East)

	10		"Hellas Sat" (39° East)

	11		"Turksat" (42° East)

	12		"Thor & IS10-02" (= Thor on 0.8° West
					& Intelsat10-02 on 1° West)

	13		"Amos" (4° West)

	14		"Atlantic Bird 3" (5° West)

	15		"Nilesat & AB4" (= Nilesat & Atlantic Bird 4 
					on 7° West)

	16		"Atlantic Bird 1" (12.5° West)

	17		"Hispasat" (30° West)


(Antenna-/LNB-numbers 18 - 32, in contrast, may still be used freely.)


Use HNFSmart2.4fix2 to adapt existing Settings-files in two steps:
  (the "satnames.ini"-file  of HNFSmart2.4fix2 must have been replaced 
   by the new one of the ToH3.4HoT11.5-package)

1.
  Those user-defined Satellite Names to which equivalent (!)
  firmware-embedded Satellite Names are available, should be replaced
  by firmware-embedded Satellite Names:
  Click on the "Antenna"-Tab and check all 32 LNBs which type
  of Satellite Name is actually in use, and change the type of name, if 
        necessary;
  Do not change those user-defined Satellite Names to which no equivalent 
  firmware-embedded Satellite Name is availabe (e. g. "Telstar 12").


2.
  The Tool "Sort LNB" ((HNFSmart2.4fix2 --> Tools --> Sort LNB) allows
  changing the relations between Antenna-/LNB-numbers and
  Satellite Names easily. Thus you can establish relations between
  Antenna-/LNB-numbers and Satellite Names in full compliance with the
  recommendations made above.
  



ToH-HoT-Team & Lombardo